|  |  |  |  |
| --- | --- | --- | --- |
| **MILAN** | | | |
| **S.no** | **Description** | **UOM** | **Specification** |
|  | Physical State / Color | - | Solid/Red |
|  | Igniter Resistance | Ohms | 0.75 – 1.20 |
|  | Head mass | g | 0.03 – 0.12 |
|  | No of Head | No’s | 2 (Double head Parallel) |
|  | Vibration | Hz | 20 - 25 |
|  | Powder Piles | A | 0.49 – 0.51 |
|  | All Fire Current (AFC) | mA | 2000mA for 10s |
|  | No Fire Current (NFC) | mA | 500mA for 300 sec |
| **KONKUR** | | | |
| **S.no** | **Description** | **UOM** | **Specification** |
|  | Physical State / Color | - | Solid/Red |
|  | Igniter Resistance | Ohms | 2.00 to 4.00 |
|  | Head mass | g | 0.03 – 0.07 |
|  | No of Head | No’s | 1 (Single Head) |
|  | Vibration | Hz | XXX |
|  | Powder Piles | A | 0.49 – 0.51 |
|  | All Fire Current (AFC) | mA | 500mA for 10sec |
|  | No Fire Current (NFC) | mA | 74 – 76mA for 300sec |